<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<library>
<packages>
<package name="USB-MICRO-SMD">
</package>
</packages>
<symbols>
<symbol name="USB_AB">
<description>USB AB, 5-pins: USBVCC, GND, D+, D-, USBID.</description>
<pin name="D+"/>
<pin name="D-"/>
<pin name="GND"/>
<pin name="USBID"/>
<pin name="VBUS"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="USB" prefix="U" uservalue="yes">
<description>This is a USB AB connector that is compatible with USB OTG. i.e. this connector can serve as a host or device</description>
<gates>
<gate name="G$1" symbol="USB_AB"/>
</gates>
<devices>
<device name="&quot;&quot;" package="USB-MICRO-SMD">
<connects>
<connect gate="G$1" pin="D+" pad="D+1"/>
<connect gate="G$1" pin="D-" pad="D-1"/>
<connect gate="G$1" pin="GND" pad="GND1"/>
<connect gate="G$1" pin="USBID" pad="ID1"/>
<connect gate="G$1" pin="VBUS" pad="VBUS1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
